|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| JOB/TASK NAME: Operation of Battery Charger  Job Safety Analysis Form | | | | PAGE 1 OF 1 | | DATE: 2/6/15 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: Grounds | | | | SUPERVISOR(S): | | ANALYSIS BY: | |
| PLANT/LOCATION: Campus | | DEPARTMENT(S): Grounds | | SHIFT (if applicable): | | APPROVED BY: Chris Gale | |
| PERSONAL PROTECTIVE EQUIPMENT: Safety Glasses | | | | | | | |
| TRAINING REQUIREMENTS: | | | | | | | |
| JOB STEPS | | | POTENTIAL HAZARDS | | ACTION/PROCEDURE TO CONTROL OR ELIMINATE | | |
| 1 | Connecting Charger to Battery | | Spark | | Connect Positive (Red) charger clip to positive post of battery | | |
| 2 | Turning Charger “On” | | Spark, Battery explosion | | Plug charger in. Make sure it is on the correct voltage setting. Turn timer to desired charge time. | | |
| 3 | Turning Charger “Off” | | Spark, Battery explosion | | Unplug charger first. Remove positive and negative charger clips from battery. Put charger back to appropriate storage spot | | |
| 4 |  | |  | |  | | |
| 5 |  | |  | |  | | |

