|  |  |  |  |
| --- | --- | --- | --- |
| JOB/TASK NAME: Operation of Battery ChargerJob Safety Analysis Form | PAGE 1 OF 1 | DATE: 2/6/15 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: Grounds | SUPERVISOR(S):  | ANALYSIS BY:  |
| PLANT/LOCATION: Campus | DEPARTMENT(S): Grounds | SHIFT (if applicable): | APPROVED BY: Chris Gale |
| PERSONAL PROTECTIVE EQUIPMENT: Safety Glasses |
| TRAINING REQUIREMENTS: |
| JOB STEPS | POTENTIAL HAZARDS | ACTION/PROCEDURE TO CONTROL OR ELIMINATE |
| 1 | Connecting Charger to Battery |  Spark | Connect Positive (Red) charger clip to positive post of battery |
| 2 | Turning Charger “On” | Spark, Battery explosion | Plug charger in. Make sure it is on the correct voltage setting. Turn timer to desired charge time. |
| 3 | Turning Charger “Off” | Spark, Battery explosion | Unplug charger first. Remove positive and negative charger clips from battery. Put charger back to appropriate storage spot |
| 4 |  |  |  |
| 5 |  |  |  |

