|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| JOB/TASK NAME:  Operating Power Edger | | | | PAGE\_\_1\_\_OF\_1\_\_ | | DATE:  12/9/2020 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB:  Supervisor’s and Students | | | | SUPERVISOR(S):  All Supervisors | | ANALYSIS BY: | |
| PLANT/LOCATION:  Campus | | DEPARTMENT(S):  Grounds | | SHIFT (if applicable): | | APPROVED BY:  Paul Snyder | |
| PERSONAL PROTECTIVE EQUIPMENT:  Eye and Ear Protection, Pruning Chaps | | | | | | | |
| TRAINING REQUIREMENTS:  Canvas Training, Plus Hands On Training | | | | | | | |
| JOB STEPS | | | POTENTIAL HAZARDS | | ACTION/PROCEDURE TO CONTROL OR ELIMINATE | | |
| 1 | Make sure fuel cap is secure | | Fire | | Hand tighten fuel cap and make sure it seals so no fuel leaks out | | |
| 2 | Start edger to make sure the blades aren’t bound together | | Edger not working properly | | If blades are not shifting back and forth, TAG IT NOT WORKING and have your supervisor or mechanic fix it. | | |
| 3 | When in use make sure pruning chaps are worn | | Bodily Harm | | Make sure cutting blades are clear of yourself, and other near you | | |
| 4 |  | |  | |  | | |
| 5 |  | |  | |  | | |



Job Safety Analysis Form