|  |  |  |  |
| --- | --- | --- | --- |
| JOB/TASK NAME:Operating Power Edger | PAGE\_\_1\_\_OF\_1\_\_ | DATE:12/9/2020 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB:Supervisor’s and Students | SUPERVISOR(S):All Supervisors | ANALYSIS BY: |
| PLANT/LOCATION:Campus | DEPARTMENT(S): Grounds | SHIFT (if applicable): | APPROVED BY:Paul Snyder |
| PERSONAL PROTECTIVE EQUIPMENT: Eye and Ear Protection, Pruning Chaps |
| TRAINING REQUIREMENTS: Canvas Training, Plus Hands On Training |
| JOB STEPS | POTENTIAL HAZARDS | ACTION/PROCEDURE TO CONTROL OR ELIMINATE |
| 1 | Make sure fuel cap is secure | Fire |  Hand tighten fuel cap and make sure it seals so no fuel leaks out |
| 2 |  Start edger to make sure the blades aren’t bound together |  Edger not working properly | If blades are not shifting back and forth, TAG IT NOT WORKING and have your supervisor or mechanic fix it. |
| 3 |  When in use make sure pruning chaps are worn |  Bodily Harm |  Make sure cutting blades are clear of yourself, and other near you  |
| 4 |   |   |   |
| 5 |   |   |   |



Job Safety Analysis Form