|  |  |  |  |
| --- | --- | --- | --- |
| JOB/TASK NAME: Use of Hand Grinder Job Safety Analysis Form | PAGE 1 OF 1 | DATE: 11/4/14 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: Grounnds | SUPERVISOR(S):  | ANALYSIS BY:  |
| PLANT/LOCATION: Campus | DEPARTMENT(S): Grounds | SHIFT (if applicable): | APPROVED BY: Chris Gale |
| PERSONAL PROTECTIVE EQUIPMENT: Eye and ear protection |
| TRAINING REQUIREMENTS: Canvas and Hands on |
| JOB STEPS | POTENTIAL HAZARDS | ACTION/PROCEDURE TO CONTROL OR ELIMINATE |
| 1 | Check cord and plug | Shock hazard | If damaged talk to electrician to see if it can be fixed, if not replace grinder |
| 2 | Check grinding wheel | Bodily Harm | If cracked or worn down replace it |
| 3 | Eye and ear protection | Bodily Harm | Make sure operator is wearing approved eye and ear protection |
| 4 |  |  |  |
| 5 |  |  |  |

