|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| JOB/TASK NAME: Operating the Man Lift  Job Safety Analysis Form | | | | PAGE 1 OF 1 | | DATE: 2/17/15 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: Dan Camp | | | | SUPERVISOR(S): Chris Gale | | ANALYSIS BY: Dan Camp | |
| PLANT/LOCATION: Campus | | DEPARTMENT(S): Grounds | | SHIFT (if applicable): | | APPROVED BY: Chris Gale | |
| PERSONAL PROTECTIVE EQUIPMENT: Harness for each person, Safety Glasses, Hard Hats, Long Sleeved Shirt | | | | | | | |
| TRAINING REQUIREMENTS: Trained on Operation of Man Lifts | | | | | | | |
| JOB STEPS | | | POTENTIAL HAZARDS | | ACTION/PROCEDURE TO CONTROL OR ELIMINATE | | |
| 1 | Start and inspect the lift | | Very few hazards exist, however, you should always be cautious when starting equipment | | Be cautious when starting or inspecting the lift | | |
| 2 | Getting in the lift and testing operation controls before starting to work | | You could fall, you could get crushed | | You need to make sure your harness is on correctly and never put your arms outside the box while operating the lift | | |
| 3 | Drive the lift to the work site | | Hitting bumps may cause the person in the lift to “pop” up. Also you could possibly hit other vehicles or buildings that could injure you and the other person. | | Always go slow. Never hit bumps going full speed, make sure your harness if on correctly. Always make sure to use extra caution while working around the public | | |
| 4 | Cutting branches out of trees | | Branches could fall and hit someone or another employee | | Always come off area that is being worked in, you should always have a spotter on the ground to watch for pedestrians and other workers. Make sure other workers are aware when you are cutting a branch so they can move out from under the lift. | | |
| 5 |  | |  | |  | | |

