|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| JOB/TASK NAME: Use of Hand Grinder  Job Safety Analysis Form | | | | PAGE 1 OF 1 | | DATE: 11/4/14 | NEW REVISED |
| EMPLOYEE(S)/POSITION(S) PERFORMING THE JOB: Grounnds | | | | SUPERVISOR(S): | | ANALYSIS BY: | |
| PLANT/LOCATION: Campus | | DEPARTMENT(S): Grounds | | SHIFT (if applicable): | | APPROVED BY: Chris Gale | |
| PERSONAL PROTECTIVE EQUIPMENT: Eye and ear protection | | | | | | | |
| TRAINING REQUIREMENTS: Canvas and Hands on | | | | | | | |
| JOB STEPS | | | POTENTIAL HAZARDS | | ACTION/PROCEDURE TO CONTROL OR ELIMINATE | | |
| 1 | Check cord and plug | | Shock hazard | | If damaged talk to electrician to see if it can be fixed, if not replace grinder | | |
| 2 | Check grinding wheel | | Bodily Harm | | If cracked or worn down replace it | | |
| 3 | Eye and ear protection | | Bodily Harm | | Make sure operator is wearing approved eye and ear protection | | |
| 4 |  | |  | |  | | |
| 5 |  | |  | |  | | |

